                                       1964  Porsche 356  SC  Coupe  by Karmann
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We are very happy to introduce this magnificent 356 SC coupe totally restored in it’s original colour of

                                                   slate grey with a dark red leather interior.
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The car was in original paint before restoration, and the colour was copied exactly to the factory paint.
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The SC was the most powerful version of the pushrod engines, only the carrera version was offering extra power.
The 4 wheel disc brake systems, introduced for the first time, is offering comfortable and extra stopping power.
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Options on this magnificent car include an original Leitz chrome luggage rack and ventilated chrome wheels 
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The panel fit is to factory standards, demonstrating the car had a good an easy and pampered life
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    Sides are straight and the doors fit in very nicely.          Chrome and strips, bumperettes, lights new or redone.
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Similar situation on the front side:  All parts, lenses, lights rubbers, chrome  are new or reconditioned
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Opening the door invites to a magnificent interior in beautiful dark red leather.  Who would not step in this car ?
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The drivers seat is even more inviting with the wooden VDM carrera steering wheel to hold.
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                                  Perfect interior finish, beautiful leather and original type carpets
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                                  Magnificent in detail:  rechromed seat hinges mean an expensive job
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The reclining Seats must give better access to the back of the car. Your choice of small seats or luggage storage. 
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                                              Seats and rails restored with the finest details
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              All new weather stripping, new aluminium profiles, every screw is new
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                                                                Check it from any angle..
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                                                         Rarely seen as refined on a 356 coupé
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                                   Clock is positioned on the right side, next to the glove box.
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                               The door jams are perfect, door panels are redone with correct screws
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                                                                             Great detailing
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             Beautiful dash with rebuild gauges, VDM steering Wheel and temperature gauges in the middle.

            Tacho up to 6.000 rpm is correct for late SC models.  Original Blaupunkt radio works very well. 
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                                               Sunvisors remade new, new headliner of course
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                           All window frames are rechromed and rebuild, new rubber everywhere.
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                                                          Hot cleaned gas tank is fully restored
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Full engine rebuilt includes new original cranckshaft and Mahle pistons to allow all original factory quotes
Original Solex carbs rebuilt by specialist Bieker.  All sheet metal powder coated.
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                                                Original  numbers  matching engine to the chassis
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                                                    An impressive view of the undercarriage
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                    Undercarriage was special soda blasted and treated with special Wurth undercoating texure
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I think it must be clear by now that this car has been exceptionally well restored, into the smallest details.
Even all the locks were rebuilt and key coded.  No money was saved and everything was done with the

care.  Few coupe to receive this attention and apart from the purchase price of many expensive parts, here

after follows  the list of the labour that was spend on the car.  The car is not cheap, but definitely worth 

                                                                           all the money !

Please call me for pricing at ++32.93.61.24.89

Thank you,

Dirk Libeert

www.classicmotoraction.com
List of work:

DISASSEMBLE BODY 

REMOVE INTERIOR COMPLETE

REMOVE ENGINE AND TRANSMISSION

REMOVE SUSPENSION

SODA BLAST UNDER CARRIAGE AND WHEEL WELLS

REUNDERCOAT WITH WURTH UNDERCOATING TEXURE

REMOVE OLD PAINT AND PREPARE FOR COMPLETE REFINISH

ALL BODY PANEL REPAIR AND PANEL FIT PRIOR TO PRIME

PAINT AND REFINISH IN ORIGINAL COLOR SLATE GREY

AUTOBAHN PAINT REFINSH SHOP IN COSTA MESA

PREPARE TRUNK FOR NEW SOUND DAMP MATERIAL

PREPARE ENGINE COMPARTMENT FOR SOUND DAMP 

CLEAN AND PREPARE ALL WIRING

DIP AND SEAL FUEL TANK 

CLEAN AND RECONDITION FUEL PET COCK

POWDER COAT SUSPENSION AND SHEET METAL

CLEAR CAD PLATE ALL HARDWARE 

REBUILD ALL BRAKE CALIPERS

GOLD ANNODIZE CALIPER PARTS PRIOR TO RECON

DISASSEMBLE ENGINE

HOT TANK ALL PARTS AND CLEAN 

INSTALL NEW MAIN BEARINGS STANDARD

INSTALL NEW GERMAN COUNTER WEIGHT CRANK

INSTALL NEW ROD BEARINGS STANDARD

INSTALL NEW CAM GEAR

INSTALL NEW WRIST PIN BUSHINGS

RECONDITION CONNECTING RODS BOTH ENDS

INSTALL NEW MAHLE PIST AND CYLS “SC”

FLY CUT HEADS AND RENEW VALVE GUIDES

FULL VALVE GRIND ON HEADS AND VALVES

FULL ENGINE GASKET KIT TOP AND BOTTOM END

INSTALL NEW MUFFLER

MACHINE AND BALANCE FLYWHEEL

INSTALL AND SET END PLAY

INSTALL NEW CLUTCH DISC

INSTALL NEW PRESSURE PLATE

INSTALL NEW THROW OUT BEARING

INSTALL ALL POWDER COAT SHEETMETAL

INSTALL BIEKER MACHINED SOLEX CARBS

INSTALL NEW SPARK PLUGS

INSTALL NEW DISTRIBUTOR CAP

INSTALL NEW POINTS

INSTALL NEW CONDENSOR

INSTALL CORRECT 6V IGINTION COIL

INSTALL CORRECT SOLEX WIRE MESH AIR FILTERS

INSTALL ALL DECALS ON ENGINE

DISASSEMBLE TRANSMISSION

INSTALL SHIFT HOUSING SHIFT BUSHING

INSTALL SHIFT ROD GUIDE BUSHING

INSTALL SHIFT COUPLER BUSHINGS 

HOT TANK AND CLEAN 

INSTALL MAINSHAFT BEARING

INSTALL PINION SHAFT BEARING

INSTALL NEW SYNCHRO RINGS

INSTALL ALL NEW GASKETS AND SEALS

INSTALL NEW CROSS SHAFT AND BUSHINGS

INSTALL NEW T.O. FORK

INSTALL REBUILT STARTER MOTOR 

INSTALL NEW LEFT AND RIGHT TRANS MOUNTS

INSTALL NEW SHIFT COUPLER 

INSTALL NEW SHIFT COUPLER BOOT

SAFETY WIRE SHIFT COUPLER SET SCREW

INSTALL NEW AXLE BOOTS

INSTALL POWDER COATED AXLE TUBES

INSTALL NEW WHEEL BEARINGS AND SEALS

REPLACE TRANSMISSION INTO CAR 

INSTALL SPRING PLATES WITH RUBBER BUSHINGS

SET VEHICLE RIDE HEIGHT

RENEW BRAKE SYSTEM

INSTALL NEW MASTER CYLINDER

INSTALL FRONT AND REAR RUBBER BRAKE HOSES

INSTALL FRONT AND REAR NEW BRAKE ROTORS

INSTALL INNER AND OUTER FRONT WHEEL BEARINGS

INSTALL NEW WHEEL SEALS

INSTALL FRONT AND REAR BRAKE CALIPERS

INSTALL NEW BRAKE PADS

INSTALL ENGINE INTO CAR

FULL INTERIOR REPLACEMENT

INSTALL NEW LEATHER SEATS

CHROME SEAT HINGES INNER AND OUTER

POWDER COAT SEAT BASES BEFORE REFINSH

INSTALL DASH PAD AND COVERING

INSTALL NEW HEADLINER

INSTALL NEW CORRECT GERMAN CARPET

INSTALL NEW DOME LIGHTS

INSTALL NEW REAR VIEW MIRROR

INSTALL REAR WINDOW DEFOGGER DIFFUSERS

INSTALL ALL GAGES REBUILT BY NORTH HOLLYWOOD SPEED

INSTALL OUTSIDE TEMP GAGE

INSTALL WOOD VDM CARRERA WHEEL

INSTALL NEW GLOVE BOX HOUSING

INSTALL RECONDITIONED LOCK ASSEMBLIES

CODE AND CUT KEYS FOR TRANS LOCK AND GLOVE BOX

INSTALL NEW DOOR PANELS LEFT AND RIGHT

INSTALL REAR JUMP SEATS

CLEAN AND RENEW WIPER MOTOR

CLEAN AND CHECK UNDER DASH WIRING

INSTALL NEW INSTRUMENT LIGHTS

INSTALL ALL NEW RUBBER SEALS ON BODY

INSTALL ALL NEW WINDOW FELT INNER AND OUTER

RECHROME QUARTER WINDOW LATCHES

RECHROME QUARTER WINDOW FRAMES

INSTALL NEW INNER AND OUTER RUBBER SEALS

RECHROME DOOR WINDOW FRAMES LEFT AND RIGHT

RECHROME WINDWINGS AND LOCK ACCESSORIES

INSTALL WINDWING SEALS

INSTALL NEW WINDSHIELD CORRECT SIGLA

INSTALL NEW WINDSHIELD RUBBER SEAL

INSTALL NEW WINDSHIELD SURROUND TRIM

INSTALL REAR WINDSCREEN

INSTALL NEW REAR WINDSCREEN SEAL

INSTALL NEW REAR SURROUND TRIM

INSTALL NEW FRONT AND REAR RUBBER FLOOR MATS

INSTALL NEW PEDAL PADS

INSTALL NEW GAS PEDAL PAD

INSTALL POWDER COATED SEAT CHASSIS 

INSTALL CAD PLATED SEAT CHANNELS

INSTALL LEFT AND RIGHT SEATS

INSTALL RADIO

INSTALL DOOR JAMB DOME LIGHT SWITCHES

INSTALL NEW DOOR SEALS LEFT AND RIGHT

INSTALL NEW SILL RUBBER 

INSTALL NEW NARROW AND WIDE CARPET TRIM

INSTALL CHROMED AND REBUILT DOOR HANDLES

INSTALL DOOR HANDLE BASE GASKETS

INSTALL NEW OUTSIDE MIRROR

REASSEMBLE BODY

INSTALL FRONT HOOD

INSTALL RECHROMED HOOD HANDLE

INSTALL NEW HOODHANDLE CREST

INSTALL NEW HOODHANDLE SEAL

INSTALL FRONT BUMPER

INSTALL POWDER COATED BUMPER BRACKETS

INSTALL FRONT BUMPER DECO TRIM

INSTALL RECHROMED BUMPER GUARDS WITH TRIM

INSTALL NEW HORN GRILLE

INSTALL NEW FOG LAMP GRILLES

INSTALL REBUILT HORNS LEFT AND RIGHT

INSTALL NEW FRONT CORNER LIGHT ASSEMBLIES

INSTALL LEFT AND RIGHT HEADLIGHT ASSEMBLIES

INSTALL REAR BUMPER

INSTALL POWDER COATED BUMPER BRACKETS

INSTALL REAR DECO STRIPS

INSTALL REAR BUMPER GUARDS

INSTALL REAR BUMPER GUARD EXHAUST HORNS

INSTALL REAR CHROME EXHAUST TIPS ON BUMPER GUARDS

INSTALL REAR CORNER BRAKE AND TURN LIGHT ASSEMBLY

INSTALL NEW REAR BACK UP LIGHT ASSEMBLY

INSTALL REAR DECKLID AND ADJUST 

INSTALL FOUR GREY REAR DECKLID BUFFERS

INSTALL RECHOMED DATE CORRECT RIMS

INSTALL NEW TIRES

INSTALL RECHROMED HUBCAPS

INSTALL NEW HUBCAP CREST

INSTALL SILVER POWDER COATED SPARE WHEEL

INSTALL NEW BATTERY

INSTALL NEW SPARE TIRE STRAP

INSTALL NEW BRAKE RESEVOIR

INSTALL NEW WINDSHIELD WASHER CANNISTER

INSTALL NEW FUSE BOX COVER

INSTALL PLASTIC GAS TANK COVER

INSTALL NEW LEITZ LUGGAGE RACK

START ENGINE AND TUNE AND ADJUST

ROAD TEST AND ADJUST

